**GENERAL**

1. The White-Light PoE illuminator shall be a solid state LED device utilizing PLATINUM Elite SMT (Surface Mount Technology) LEDs, light intensifying optics and light shaping holographic diffuser with current controlled LEDs providing at least 10 years illumination life (44,000hrs night time use).
2. The illuminator shall be powered from a PoE input and requires a 60W PoE++ (4-pair PoE) input.
3. The illuminator shall include an adjustable photocell for automatic on/off operation.
4. The PoE illuminator shall plug in to an existing PoE enabled network infrastructure without the need for an additional power supply unit.
5. White-Light models shall be available with a colour temperature of ~6000k. Other colour temperatures available.
6. The PoE illuminator shall offer a Premium version which will include options for 24V DC input, telemetry control input (volt-free or TTL input), and volt-free photocell-following output.
7. The LED illuminator shall be vandal resistant and manufactured using high impact polycarbonate lensing and shall incorporate an aluminum extruded heat sink to aid LED life expectancy.
8. The illuminator shall have an IP66 rating as a minimum.
9. The illuminator shall have an operational temperature range between -50 to 50˚C (-58 to 122°F).
10. The illuminator shall be CE and FCC approved.
11. The illuminator shall incorporate hot-spot reduction (HRT) technology.
12. The illuminator shall incorporate status LEDs indicating correct input voltage and receipt of valid commands.
13. The illuminator shall make use of interchangeable diffuser-lenses permitting optional angles of 10°, 35°, 60°, 80°, 120° and custom diffuser-lenses as an option.
14. The illuminator shall be controllable using a hand-held remote control permitting remote adjustment of the following parameters:
    1. Power Select – 20%, 40%, 60%, 80% and 100% of power
    2. Photocell Adjust – 3 sensitivity levels
    3. Photocell Disable
    4. Timer Setting – telemetry-triggered, pre-determined on period for selectable periods of 1, 3, 10 and 30 minutes and timer disable.
    5. Remote Control Set-up Disable
    6. Restore Factory Defaults (excluding PIN)
    7. Remote Dimming
    8. LED Status Indicators on/off
    9. Assign a security PIN

1. The illuminator shall be controllable via manual input buttons on the illuminator of the following functions:
   1. Power Select – 20%, 40%, 60%, 80% and 100% of power
   2. Photocell Adjust – 3 sensitivity levels
   3. Photocell Disable
   4. LED Status Indicators on/off
   5. Restore Factory Defaults (excluding PIN reset)
   6. Remote Control Set-up Disable
   7. Manual Button Disable
   8. Restore Factory Defaults (including PIN reset)
2. Programming inputs on both the remote control and on the illuminator can be disabled if required.
3. The illuminator can be assigned a PIN code using the remote control to lock in settings and limit access.
4. The illuminator shall comply with the POWERS lighting standard and the manufacturer shall guarantee that the White-Light illuminator will provide a minimum of 3 Lux power on scene at the maximum quoted distance.
5. The illuminator shall be covered by a manufacturer’s warranty of 5 years

**TECHNICAL SPECIFICATIONS**

1. The illuminator shall meet or exceed the following specifications:
   1. Max. lighting distance: 180m (591ft)
   2. Total Lumens: 3727 lm per luminaire
   3. Angle of Illumination: 10, 35, 60, 80, 120, degrees, adjustable from a

single unit

* 1. Optics: PLATINUM Elite SMT LEDs
  2. Wavelength: White-Light
  3. Colour Temperature: 6000K~
  4. Colour Reproduction Index: >70
  5. Power on Scene

at max distance: At least 3 Lux

* 1. Consumption: 47 watts
  2. Input: 60W PoE++ (4-pair PoE)   
      (and 24V DC on Premium versions)
  3. Weight: 1.65kg (3.6lbs)
  4. Ingress Protection Rating: IP66
  5. Operating Temperature: -50°C to + 50⁰C (-58 to 122°F)
  6. Colour: Silver (RAL 9006) as standard. Other colours available

to order

* 1. Dimensions: 135mm x 180mm x 68.2mm (5” x 7” x 2.6”)

* 1. Cable: 1x Cat5
  2. Control: Manual buttons or remote control

1. The illuminator shall be covered by a manufacturer’s warranty of 5 years.
2. The illuminator shall be available with full specification data based on the POWERS lighting standard for video surveillance.
3. The illuminator shall be available with additional VARIO Universal Bracketry (VUB), to accommodate for the mounting of multiple LED panels at various horizontal and vertical tilts.
4. The White-Light illuminator shall be the VAR2-POE-w8-1 manufactured by Raytec or an approved equivalent.